Bath/Bar Sink Installation

There is more than one way to install your bathroom sink. However, we recommend using a clear, acid free silicone such as a GEII (General Electric Roman numeral 2) silicone. You can also use clips to undermount the sink. You can find these items at your local hardware store or order them online. As for the installation, we have listed instructions below:

1. Be sure to clean the underside of your countertop and the rim of the copper sink with rubbing alcohol. Remove any dust or debris that could get trapped beneath the sink's rim.
2. Place sink upside down on countertop and mark countertop by tracing edge of sink basin.
3. Apply a bead of silicone around the sink cutout on the counter. Make sure the bead is continuous, as the weight of the sink's rim will push it out, helping to seal the rim against moisture and leaks.
4. You may want to use a level to be sure the front, back, and both sides of your sink are even when pressing down to affix the sink to your countertop.
5. Use clamps to secure the basin under the countertop and hold the sink in place while the silicone is drying.
6. Carefully remove any excess silicone and allow silicone to dry completely. Excess silicone will push out from under the rim; use your index finger to smooth the edge of the silicone against the edge of the sink's rim. Allow the silicone to dry for 24 hours, once silicone is dry you can remove the clamps.
7. When cleaning up after installations, do not use abrasive cleaners.